<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<library>
<packages>
<package name="OPEN">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="LOAD_GCPW">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="LOAD_MICROSTRIP">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="U.FL">
<description>U.FL.</description>
</package>
<package name="SHORT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_25_OHM_TLINE_SHORT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_25_OHM_LEFT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_25_OHM_RIGHT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_25_OHM_TLINE_LONG">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_25_OHM_TEE">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_25_OHM_0402_SHUNT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_25_OHM_0402_SERIES">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_25_OHM_THRU">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_35_OHM_TLINE_SHORT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_35_OHM_LEFT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_35_OHM_RIGHT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_35_OHM_TLINE_LONG">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_35_OHM_TEE">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_35_OHM_0402_SHUNT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_35_OHM_0402_SERIES">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_35_OHM_THRU">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_50_OHM_TLINE_SHORT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_50_OHM_LEFT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_50_OHM_RIGHT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_50_OHM_TLINE_LONG">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_50_OHM_TEE">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_50_OHM_0402_SHUNT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_50_OHM_0402_SERIES">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_50_OHM_THRU">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_70_OHM_TLINE_SHORT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_70_OHM_LEFT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_70_OHM_RIGHT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_70_OHM_TLINE_LONG">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_70_OHM_TEE">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_70_OHM_0402_SHUNT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_70_OHM_0402_SERIES">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_70_OHM_THRU">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_100_OHM_TLINE_SHORT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_100_OHM_LEFT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_100_OHM_RIGHT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_100_OHM_TLINE_LONG">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_100_OHM_TEE">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_100_OHM_0402_SHUNT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_100_OHM_0402_SERIES">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="GCPW_100_OHM_THRU">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_25_OHM_TLINE_SHORT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_25_OHM_LEFT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_25_OHM_RIGHT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_25_OHM_TLINE_LONG">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_25_OHM_TEE">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_25_OHM_0402_SHUNT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_25_OHM_0402_SERIES">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_25_OHM_THRU">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_35_OHM_TLINE_SHORT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_35_OHM_LEFT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_35_OHM_RIGHT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_35_OHM_TLINE_LONG">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_35_OHM_TEE">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_35_OHM_0402_SHUNT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_35_OHM_0402_SERIES">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_35_OHM_THRU">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_50_OHM_TLINE_SHORT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_50_OHM_LEFT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_50_OHM_RIGHT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_50_OHM_TLINE_LONG">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_50_OHM_TEE">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_50_OHM_0402_SHUNT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_50_OHM_0402_SERIES">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_50_OHM_THRU">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_70_OHM_TLINE_SHORT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_70_OHM_LEFT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_70_OHM_RIGHT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_70_OHM_TLINE_LONG">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_70_OHM_TEE">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_70_OHM_0402_SHUNT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_70_OHM_0402_SERIES">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_70_OHM_THRU">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_100_OHM_TLINE_SHORT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_100_OHM_LEFT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_100_OHM_RIGHT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_100_OHM_TLINE_LONG">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_100_OHM_TEE">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_100_OHM_0402_SHUNT">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_100_OHM_0402_SERIES">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
<package name="MICROSTRIP_100_OHM_THRU">
<description>transmission line (Dk = 3.45 @ 10GHz, PCB thickness=0.5, I-TERA-MT-RF)</description>
</package>
</packages>
<symbols>
<symbol name="U.FL">
<pin name="GND@0"/>
<pin name="SIGNAL"/>
<pin name="GND@1"/>
</symbol>
<symbol name="TLINE_SHORT">
<pin name="1"/>
<pin name="2"/>
<pin name="GND"/>
</symbol>
<symbol name="LEFT">
<pin name="2"/>
<pin name="1"/>
<pin name="GND"/>
</symbol>
<symbol name="RIGHT">
<pin name="2"/>
<pin name="1"/>
<pin name="GND"/>
</symbol>
<symbol name="TEE">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="GND"/>
</symbol>
<symbol name="TLINE_LONG">
<pin name="1"/>
<pin name="2"/>
<pin name="GND"/>
</symbol>
<symbol name="0402_SERIES">
<pin name="1"/>
<pin name="2"/>
<pin name="GND"/>
</symbol>
<symbol name="0402_SHUNT">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="GND"/>
</symbol>
<symbol name="SHORT">
<pin name="GND@0"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@5"/>
</symbol>
<symbol name="THRU">
<pin name="GND@0"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND"/>
</symbol>
<symbol name="OPEN">
<pin name="GND@0"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
</symbol>
<symbol name="LOAD">
<pin name="GND@0"/>
<pin name="GND@1"/>
<pin name="GND@3"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="OPEN" prefix="X">
<gates>
<gate name="G$1" symbol="OPEN"/>
</gates>
<devices>
<device name="" package="OPEN">
<connects>
<connect gate="G$1" pin="GND@0" pad="1 2"/>
<connect gate="G$1" pin="GND@1" pad="3 4"/>
<connect gate="G$1" pin="GND@2" pad="5 6"/>
<connect gate="G$1" pin="GND@3" pad="7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOAD_GCPW" prefix="X">
<description>Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="LOAD"/>
</gates>
<devices>
<device name="" package="LOAD_GCPW">
<connects>
<connect gate="G$1" pin="GND@0" pad="P$1"/>
<connect gate="G$1" pin="GND@1" pad="P$2"/>
<connect gate="G$1" pin="GND@3" pad="P$6 P$7 P$8 P$9 P$10 P$11 P$12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOAD_MICROSTRIP" prefix="X">
<description>Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="LOAD"/>
</gates>
<devices>
<device name="" package="LOAD_MICROSTRIP">
<connects>
<connect gate="G$1" pin="GND@0" pad="P$1"/>
<connect gate="G$1" pin="GND@1" pad="P$2"/>
<connect gate="G$1" pin="GND@3" pad="P$6 P$7 P$8 P$9 P$10 P$11 P$12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SHORT" prefix="X">
<description>Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="SHORT"/>
</gates>
<devices>
<device name="" package="SHORT">
<connects>
<connect gate="G$1" pin="GND@0" pad="P$1"/>
<connect gate="G$1" pin="GND@1" pad="P$2"/>
<connect gate="G$1" pin="GND@2" pad="P$5"/>
<connect gate="G$1" pin="GND@3" pad="P$6"/>
<connect gate="G$1" pin="GND@5" pad="P$3 P$7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="U.FL" prefix="J" uservalue="yes">
<description>SMD antenna connector- WRL-09144</description>
<gates>
<gate name="G$1" symbol="U.FL"/>
</gates>
<devices>
<device name="" package="U.FL">
<connects>
<connect gate="G$1" pin="GND@0" pad="P$1"/>
<connect gate="G$1" pin="GND@1" pad="P$2"/>
<connect gate="G$1" pin="SIGNAL" pad="P$3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09193"/>
<attribute name="VALUE" value="U.FL"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_25_OHM_TLINE_SHORT" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE;
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_SHORT"/>
</gates>
<devices>
<device name="" package="GCPW_25_OHM_TLINE_SHORT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.753"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="ZO" value="25 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_25_OHM_L" prefix="X">
<description>Grounded Coplanar Waveguide Line - left;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="LEFT"/>
</gates>
<devices>
<device name="" package="GCPW_25_OHM_LEFT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.753"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="25 Ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_25_OHM_R" prefix="X">
<description>Grounded Coplanar Waveguide Line - right;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="RIGHT"/>
</gates>
<devices>
<device name="" package="GCPW_25_OHM_RIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.753"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="ZO" value="25 Ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_25_OHM_TLINE_LONG" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE, long; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_LONG"/>
</gates>
<devices>
<device name="" package="GCPW_25_OHM_TLINE_LONG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.753"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="ZO" value="25 Ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_25_OHM_TJUNCTION" prefix="X">
<description>Grounded Coplanar Waveguide - T JUNCTION, long; Relative dielectric constant = 3.45; Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TEE"/>
</gates>
<devices>
<device name="" package="GCPW_25_OHM_TEE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.753"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="25 Ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_25_OHM_SERIES_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - series cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SERIES"/>
</gates>
<devices>
<device name="" package="GCPW_25_OHM_0402_SERIES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.753"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="25 Ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_25_OHM_SHUNT_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - shunt cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SHUNT"/>
</gates>
<devices>
<device name="" package="GCPW_25_OHM_0402_SHUNT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.753"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="25 Ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_25_OHM_THRU" prefix="X">
<description>Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="THRU"/>
</gates>
<devices>
<device name="" package="GCPW_25_OHM_THRU">
<connects>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
<connect gate="G$1" pin="GND@0" pad="P$1"/>
<connect gate="G$1" pin="GND@1" pad="P$2"/>
<connect gate="G$1" pin="GND@2" pad="P$5"/>
<connect gate="G$1" pin="GND@3" pad="P$6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.753"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="25 Ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_35_OHM_TLINE_SHORT" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE;
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_SHORT"/>
</gates>
<devices>
<device name="" package="GCPW_35_OHM_TLINE_SHORT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.561"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="ZO" value="sqrt(25*50) Ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_35_OHM_L" prefix="X">
<description>Grounded Coplanar Waveguide Line - left;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="LEFT"/>
</gates>
<devices>
<device name="" package="GCPW_35_OHM_LEFT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.561"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="sqrt(25*50) Ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_35_OHM_R" prefix="X">
<description>Grounded Coplanar Waveguide Line - right;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="RIGHT"/>
</gates>
<devices>
<device name="" package="GCPW_35_OHM_RIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.561"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="ZO" value="sqrt(25*50) Ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_35_OHM_TLINE_LONG" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE, long; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_LONG"/>
</gates>
<devices>
<device name="" package="GCPW_35_OHM_TLINE_LONG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.561"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="ZO" value="sqrt(25*50) Ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_35_OHM_TJUNCTION" prefix="X">
<description>Grounded Coplanar Waveguide - T JUNCTION, long; Relative dielectric constant = 3.45; Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TEE"/>
</gates>
<devices>
<device name="" package="GCPW_35_OHM_TEE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4 5 6 7 8 9 10 11 12 13 14" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.561"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="sqrt(25*50) Ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_35_OHM_SERIES_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - series cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SERIES"/>
</gates>
<devices>
<device name="" package="GCPW_35_OHM_0402_SERIES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.561"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="sqrt(25*50) Ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_35_OHM_SHUNT_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - shunt cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SHUNT"/>
</gates>
<devices>
<device name="" package="GCPW_35_OHM_0402_SHUNT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.561"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="sqrt(25*50) Ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_35_OHM_THRU" prefix="X">
<description>Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="THRU"/>
</gates>
<devices>
<device name="" package="GCPW_35_OHM_THRU">
<connects>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
<connect gate="G$1" pin="GND@0" pad="P$1"/>
<connect gate="G$1" pin="GND@1" pad="P$2"/>
<connect gate="G$1" pin="GND@2" pad="P$5"/>
<connect gate="G$1" pin="GND@3" pad="P$6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.561"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="ZO" value="sqrt(25*50) Ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_50_OHM_TLINE_SHORT" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE;
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_SHORT"/>
</gates>
<devices>
<device name="" package="GCPW_50_OHM_TLINE_SHORT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.46"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="ZO" value="50 Ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_50_OHM_L" prefix="X">
<description>Grounded Coplanar Waveguide Line - left;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="LEFT"/>
</gates>
<devices>
<device name="" package="GCPW_50_OHM_LEFT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.46"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="50 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_50_OHM_R" prefix="X">
<description>Grounded Coplanar Waveguide Line - right;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="RIGHT"/>
</gates>
<devices>
<device name="" package="GCPW_50_OHM_RIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.46"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="ZO" value="50 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_50_OHM_TLINE_LONG" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE, long; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_LONG"/>
</gates>
<devices>
<device name="" package="GCPW_50_OHM_TLINE_LONG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.46"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="ZO" value="50 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_50_OHM_TJUNCTION" prefix="X">
<description>Grounded Coplanar Waveguide - T JUNCTION, long; Relative dielectric constant = 3.45; Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TEE"/>
</gates>
<devices>
<device name="" package="GCPW_50_OHM_TEE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4 5 6 7 8 9 10 11 12 13 14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.46"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="50 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_50_OHM_SERIES_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - series cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SERIES"/>
</gates>
<devices>
<device name="" package="GCPW_50_OHM_0402_SERIES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.46"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="50 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_50_OHM_SHUNT_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - shunt cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SHUNT"/>
</gates>
<devices>
<device name="" package="GCPW_50_OHM_0402_SHUNT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.46"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="50 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_50_OHM_THRU" prefix="X">
<description>Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="THRU"/>
</gates>
<devices>
<device name="" package="GCPW_50_OHM_THRU">
<connects>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
<connect gate="G$1" pin="GND@0" pad="P$1"/>
<connect gate="G$1" pin="GND@1" pad="P$2"/>
<connect gate="G$1" pin="GND@2" pad="P$5"/>
<connect gate="G$1" pin="GND@3" pad="P$6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.46"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="50 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_70_OHM_TLINE_SHORT" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE;
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_SHORT"/>
</gates>
<devices>
<device name="" package="GCPW_70_OHM_TLINE_SHORT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.34"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="ZO" value="sqrt(50*100) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_70_OHM_L" prefix="X">
<description>Grounded Coplanar Waveguide Line - left;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="LEFT"/>
</gates>
<devices>
<device name="" package="GCPW_70_OHM_LEFT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.34"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="sqrt(50*100) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_70_OHM_R" prefix="X">
<description>Grounded Coplanar Waveguide Line - right;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="RIGHT"/>
</gates>
<devices>
<device name="" package="GCPW_70_OHM_RIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.34"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="sqrt(50*100) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_70_OHM_TLINE_LONG" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE, long; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_LONG"/>
</gates>
<devices>
<device name="" package="GCPW_70_OHM_TLINE_LONG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.34"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="sqrt(50*100) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_70_OHM_TJUNCTION" prefix="X">
<description>Grounded Coplanar Waveguide - T JUNCTION, long; Relative dielectric constant = 3.45; Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TEE"/>
</gates>
<devices>
<device name="" package="GCPW_70_OHM_TEE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4 5 6 7 8 9 10 11 12 13 14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.34"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="sqrt(50*100) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_70_OHM_SERIES_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - series cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SERIES"/>
</gates>
<devices>
<device name="" package="GCPW_70_OHM_0402_SERIES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.34"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="sqrt(50*100) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_70_OHM_SHUNT_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - shunt cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SHUNT"/>
</gates>
<devices>
<device name="" package="GCPW_70_OHM_0402_SHUNT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.34"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="sqrt(50*100) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_70_OHM_THRU" prefix="X">
<description>Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="THRU"/>
</gates>
<devices>
<device name="" package="GCPW_70_OHM_THRU">
<connects>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
<connect gate="G$1" pin="GND@0" pad="P$1"/>
<connect gate="G$1" pin="GND@1" pad="P$2"/>
<connect gate="G$1" pin="GND@2" pad="P$5"/>
<connect gate="G$1" pin="GND@3" pad="P$6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.34"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="sqrt(50*100) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_100_OHM_TLINE_SHORT" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE;
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_SHORT"/>
</gates>
<devices>
<device name="" package="GCPW_100_OHM_TLINE_SHORT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.276"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="100 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_100_OHM_L" prefix="X">
<description>Grounded Coplanar Waveguide Line - left;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="LEFT"/>
</gates>
<devices>
<device name="" package="GCPW_100_OHM_LEFT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.276"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="100 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_100_OHM_R" prefix="X">
<description>Grounded Coplanar Waveguide Line - right;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="RIGHT"/>
</gates>
<devices>
<device name="" package="GCPW_100_OHM_RIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.276"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="100 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_100_OHM_TLINE_LONG" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE, long; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_LONG"/>
</gates>
<devices>
<device name="" package="GCPW_100_OHM_TLINE_LONG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.276"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="100 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_100_OHM_TJUNCTION" prefix="X">
<description>Grounded Coplanar Waveguide - T JUNCTION, long; Relative dielectric constant = 3.45; Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TEE"/>
</gates>
<devices>
<device name="" package="GCPW_100_OHM_TEE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4 5 6 7 8 9 10 11 12 13 14"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.276"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="100 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_100_OHM_SERIES_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - series cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SERIES"/>
</gates>
<devices>
<device name="" package="GCPW_100_OHM_0402_SERIES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.276"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="100 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_100_OHM_SHUNT_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - shunt cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SHUNT"/>
</gates>
<devices>
<device name="" package="GCPW_100_OHM_0402_SHUNT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.276"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="100 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_GCPW_100_OHM_THRU" prefix="X">
<description>Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="THRU"/>
</gates>
<devices>
<device name="" package="GCPW_100_OHM_THRU">
<connects>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
<connect gate="G$1" pin="GND@0" pad="P$1"/>
<connect gate="G$1" pin="GND@1" pad="P$2"/>
<connect gate="G$1" pin="GND@2" pad="P$5"/>
<connect gate="G$1" pin="GND@3" pad="P$6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="E_EFF" value="2.276"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="ZO" value="100 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_25_OHM_TLINE_SHORT" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE;
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_SHORT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_25_OHM_TLINE_SHORT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="25 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_25_OHM_L" prefix="X">
<description>Grounded Coplanar Waveguide Line - left;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="LEFT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_25_OHM_LEFT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="25 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_25_OHM_R" prefix="X">
<description>Grounded Coplanar Waveguide Line - right;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="RIGHT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_25_OHM_RIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="25 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_25_OHM_TLINE_LONG" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE, long; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_LONG"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_25_OHM_TLINE_LONG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9 P$10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="25 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_25_OHM_TJUNCTION" prefix="X">
<description>Grounded Coplanar Waveguide - T JUNCTION, long; Relative dielectric constant = 3.45; Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TEE"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_25_OHM_TEE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="25 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_25_OHM_SERIES_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - series cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SERIES"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_25_OHM_0402_SERIES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9 P$10 P$11"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="25 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_25_OHM_SHUNT_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - shunt cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SHUNT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_25_OHM_0402_SHUNT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="25 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_25_OHM_THRU" prefix="X">
<description>Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="THRU"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_25_OHM_THRU">
<connects>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 P$9 P$10 P$11 P$12 P$13 P$14 P$15 P$16 P$17 P$18 P$19 P$20"/>
<connect gate="G$1" pin="GND@0" pad="P$1"/>
<connect gate="G$1" pin="GND@1" pad="P$2"/>
<connect gate="G$1" pin="GND@2" pad="P$5"/>
<connect gate="G$1" pin="GND@3" pad="P$6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="25 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_35_OHM_TLINE_SHORT" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE;
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_SHORT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_35_OHM_TLINE_SHORT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="sqrt(25*50) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_35_OHM_L" prefix="X">
<description>Grounded Coplanar Waveguide Line - left;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="LEFT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_35_OHM_LEFT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="sqrt(25*50) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_35_OHM_R" prefix="X">
<description>Grounded Coplanar Waveguide Line - right;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="RIGHT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_35_OHM_RIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="sqrt(25*50) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_35_OHM_TLINE_LONG" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE, long; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_LONG"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_35_OHM_TLINE_LONG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9 P$10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="sqrt(25*50) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_35_OHM_TJUNCTION" prefix="X">
<description>Grounded Coplanar Waveguide - T JUNCTION, long; Relative dielectric constant = 3.45; Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TEE"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_35_OHM_TEE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="sqrt(25*50) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_35_OHM_SERIES_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - series cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SERIES"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_35_OHM_0402_SERIES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9 P$10 P$11"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="sqrt(25*50) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_35_OHM_SHUNT_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - shunt cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SHUNT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_35_OHM_0402_SHUNT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="GND" pad="P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9 P$10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="sqrt(25*50) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_35_OHM_THRU" prefix="X">
<description>Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="THRU"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_35_OHM_THRU">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18"/>
<connect gate="G$1" pin="GND@0" pad="P$1"/>
<connect gate="G$1" pin="GND@1" pad="P$2"/>
<connect gate="G$1" pin="GND@2" pad="P$5"/>
<connect gate="G$1" pin="GND@3" pad="P$6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="sqrt(25*50) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_50_OHM_TLINE_SHORT" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE;
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_SHORT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_50_OHM_TLINE_SHORT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="50 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_50_OHM_L" prefix="X">
<description>Grounded Coplanar Waveguide Line - left;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="LEFT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_50_OHM_LEFT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4 P$5 P$7 P$8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="50 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_50_OHM_R" prefix="X">
<description>Grounded Coplanar Waveguide Line - right;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="RIGHT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_50_OHM_RIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4 P$5 P$7 P$8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="50 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_50_OHM_TLINE_LONG" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE, long; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_LONG"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_50_OHM_TLINE_LONG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9 P$10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="50 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_50_OHM_TJUNCTION" prefix="X">
<description>Grounded Coplanar Waveguide - T JUNCTION, long; Relative dielectric constant = 3.45; Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TEE"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_50_OHM_TEE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="50 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_50_OHM_SERIES_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - series cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SERIES"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_50_OHM_0402_SERIES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9 P$10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="50 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_50_OHM_SHUNT_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - shunt cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SHUNT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_50_OHM_0402_SHUNT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="50 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_50_OHM_THRU" prefix="X">
<description>Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="THRU"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_50_OHM_THRU">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18"/>
<connect gate="G$1" pin="GND@0" pad="P$1"/>
<connect gate="G$1" pin="GND@1" pad="P$2"/>
<connect gate="G$1" pin="GND@2" pad="P$5"/>
<connect gate="G$1" pin="GND@3" pad="P$6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="50 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_70_OHM_TLINE_SHORT" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE;
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_SHORT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_70_OHM_TLINE_SHORT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5mm"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="sqrt(50*100) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_70_OHM_L" prefix="X">
<description>Grounded Coplanar Waveguide Line - left;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="LEFT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_70_OHM_LEFT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="sqrt(50*100) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_70_OHM_R" prefix="X">
<description>Grounded Coplanar Waveguide Line - right;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="RIGHT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_70_OHM_RIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="sqrt(50*100) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_70_OHM_TLINE_LONG" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE, long; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_LONG"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_70_OHM_TLINE_LONG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="sqrt(50*100) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_70_OHM_TJUNCTION" prefix="X">
<description>Grounded Coplanar Waveguide - T JUNCTION, long; Relative dielectric constant = 3.45; Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TEE"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_70_OHM_TEE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="sqrt(50*100) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_70_OHM_SERIES_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - series cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SERIES"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_70_OHM_0402_SERIES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9 P$10 P$11"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="sqrt(50*100) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_70_OHM_SHUNT_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - shunt cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SHUNT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_70_OHM_0402_SHUNT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="sqrt(50*100) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_70_OHM_THRU" prefix="X">
<description>Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="THRU"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_70_OHM_THRU">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18"/>
<connect gate="G$1" pin="GND@0" pad="P$1"/>
<connect gate="G$1" pin="GND@1" pad="P$2"/>
<connect gate="G$1" pin="GND@2" pad="P$5"/>
<connect gate="G$1" pin="GND@3" pad="P$6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="sqrt(50*100) ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_100_OHM_TLINE_SHORT" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE;
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_SHORT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_100_OHM_TLINE_SHORT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="100 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_100_OHM_L" prefix="X">
<description>Grounded Coplanar Waveguide Line - left;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="LEFT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_100_OHM_LEFT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="100 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_100_OHM_R" prefix="X">
<description>Grounded Coplanar Waveguide Line - right;
Relative dielectric constant = 3.45;
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="RIGHT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_100_OHM_RIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="100 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_100_OHM_TLINE_LONG" prefix="X">
<description>Grounded Coplanar Waveguide Line - TLINE, long; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TLINE_LONG"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_100_OHM_TLINE_LONG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="100 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_100_OHM_TJUNCTION" prefix="X">
<description>Grounded Coplanar Waveguide - T JUNCTION, long; Relative dielectric constant = 3.45; Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="TEE"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_100_OHM_TEE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="4 5 6 7 8 9 10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="100 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_100_OHM_SERIES_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - series cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SERIES"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_100_OHM_0402_SERIES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 10 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="100 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_100_OHM_SHUNT_0402" prefix="X">
<description>Grounded Coplanar Waveguide Line - shunt cap 0402; 
Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="0402_SHUNT"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_100_OHM_0402_SHUNT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="GND" pad="3 4 5 6 7 8 9 11 12"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="VALUE" value="xx pF"/>
<attribute name="ZO" value="100 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHIPDESIGN_MICROSTRIP_100_OHM_THRU" prefix="X">
<description>Relative dielectric constant = 3.45; 
Thickness of dielectric = 0.5mm.</description>
<gates>
<gate name="G$1" symbol="THRU"/>
</gates>
<devices>
<device name="" package="MICROSTRIP_100_OHM_THRU">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18"/>
<connect gate="G$1" pin="GND@0" pad="P$1"/>
<connect gate="G$1" pin="GND@1" pad="P$2"/>
<connect gate="G$1" pin="GND@2" pad="P$5"/>
<connect gate="G$1" pin="GND@3" pad="P$6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value="I-TERA-MT-RF"/>
<attribute name="DK" value="3.45"/>
<attribute name="PCB_THICKNESS" value="0.5MM"/>
<attribute name="TRACK_THICKNESS" value="35um"/>
<attribute name="ZO" value="100 ohms"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
