<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<library>
<packages>
<package name="USBULC6">
</package>
<package name="SOT23-6">
</package>
<package name="DFN-8">
</package>
<package name="SPBT2632C2A">
</package>
<package name="LPS25H">
</package>
<package name="SO-16">
</package>
<package name="SOIC-16">
</package>
<package name="DPAK">
</package>
</packages>
<symbols>
<symbol name="USBULC6">
<pin name="D-@1"/>
<pin name="D+@1"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="D+@2"/>
<pin name="D-@2"/>
</symbol>
<symbol name="ST1S10PUR">
<pin name="VIN_SW"/>
<pin name="EN"/>
<pin name="VIN_A"/>
<pin name="SYNC"/>
<pin name="AGND"/>
<pin name="PGND"/>
<pin name="FB"/>
<pin name="SW"/>
</symbol>
<symbol name="ST3232">
<pin name="VCC"/>
<pin name="R1OUT"/>
<pin name="T1IN"/>
<pin name="R2OUT"/>
<pin name="T2IN"/>
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="GND"/>
<pin name="V-"/>
<pin name="V+"/>
<pin name="T2OUT"/>
<pin name="R2IN"/>
<pin name="T1OUT"/>
<pin name="R1IN"/>
<pin name="C1-"/>
<pin name="C1+"/>
</symbol>
<symbol name="SPBT2632C2A">
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="GPIO6"/>
<pin name="LPO"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="BOOT"/>
<pin name="!RESET"/>
<pin name="CTS"/>
<pin name="RTS"/>
<pin name="RXD"/>
<pin name="TXD"/>
</symbol>
<symbol name="LPS25H">
<pin name="VCCIO"/>
<pin name="SCL/SPC"/>
<pin name="RES"/>
<pin name="SDA/SDI/SDO"/>
<pin name="SDO/SAO"/>
<pin name="CS"/>
<pin name="INT1"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="VCC"/>
</symbol>
<symbol name="VREG">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="ULN2003">
<pin name="IN1"/>
<pin name="IN2"/>
<pin name="IN3"/>
<pin name="IN4"/>
<pin name="IN5"/>
<pin name="IN6"/>
<pin name="IN7"/>
<pin name="GND"/>
<pin name="COM"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
<pin name="OUT5"/>
<pin name="OUT6"/>
<pin name="OUT7"/>
</symbol>
<symbol name="NPN">
<pin name="B"/>
<pin name="C"/>
<pin name="E"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ST3232" prefix="U">
<gates>
<gate name="G$1" symbol="ST3232"/>
</gates>
<devices>
<device name="CDR" package="SOIC-16">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USBULC6" prefix="U">
<description>&lt;b&gt; 2-line STMicroelectronics IPAD Ultra Low Capacitance TVS Diode for high speed USB. &lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="USBULC6"/>
</gates>
<devices>
<device name="" package="SOT23-6">
<connects>
<connect gate="G$1" pin="D+@1" pad="3"/>
<connect gate="G$1" pin="D+@2" pad="4"/>
<connect gate="G$1" pin="D-@1" pad="1"/>
<connect gate="G$1" pin="D-@2" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ST1S10PUR" prefix="U">
<gates>
<gate name="G$1" symbol="ST1S10PUR"/>
</gates>
<devices>
<device name="" package="DFN-8">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="PGND" pad="8 EP"/>
<connect gate="G$1" pin="SW" pad="7"/>
<connect gate="G$1" pin="SYNC" pad="5"/>
<connect gate="G$1" pin="VIN_A" pad="1"/>
<connect gate="G$1" pin="VIN_SW" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPBT2632C2A" prefix="U">
<gates>
<gate name="G$1" symbol="SPBT2632C2A"/>
</gates>
<devices>
<device name="" package="SPBT2632C2A">
<connects>
<connect gate="G$1" pin="!RESET" pad="10"/>
<connect gate="G$1" pin="BOOT" pad="9"/>
<connect gate="G$1" pin="CTS" pad="11"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="GPIO0" pad="1"/>
<connect gate="G$1" pin="GPIO1" pad="2"/>
<connect gate="G$1" pin="GPIO2" pad="3"/>
<connect gate="G$1" pin="GPIO3" pad="4"/>
<connect gate="G$1" pin="GPIO4" pad="5"/>
<connect gate="G$1" pin="GPIO5" pad="6"/>
<connect gate="G$1" pin="GPIO6" pad="16"/>
<connect gate="G$1" pin="LPO" pad="15"/>
<connect gate="G$1" pin="RTS" pad="12"/>
<connect gate="G$1" pin="RXD" pad="13"/>
<connect gate="G$1" pin="TXD" pad="14"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPS25H" prefix="U">
<gates>
<gate name="G$1" symbol="LPS25H"/>
</gates>
<devices>
<device name="" package="LPS25H">
<connects>
<connect gate="G$1" pin="CS" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="INT1" pad="7"/>
<connect gate="G$1" pin="RES" pad="3"/>
<connect gate="G$1" pin="SCL/SPC" pad="2"/>
<connect gate="G$1" pin="SDA/SDI/SDO" pad="4"/>
<connect gate="G$1" pin="SDO/SAO" pad="5"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="VCCIO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LD1117" prefix="U">
<gates>
<gate name="G$1" symbol="VREG"/>
</gates>
<devices>
<device name="ADT33TR" package="DPAK">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="TAB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ULN2003" prefix="U">
<gates>
<gate name="G$1" symbol="ULN2003"/>
</gates>
<devices>
<device name="ADR2G" package="SOIC-16">
<connects>
<connect gate="G$1" pin="COM" pad="9"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="2"/>
<connect gate="G$1" pin="IN3" pad="3"/>
<connect gate="G$1" pin="IN4" pad="4"/>
<connect gate="G$1" pin="IN5" pad="5"/>
<connect gate="G$1" pin="IN6" pad="6"/>
<connect gate="G$1" pin="IN7" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="16"/>
<connect gate="G$1" pin="OUT2" pad="15"/>
<connect gate="G$1" pin="OUT3" pad="14"/>
<connect gate="G$1" pin="OUT4" pad="13"/>
<connect gate="G$1" pin="OUT5" pad="12"/>
<connect gate="G$1" pin="OUT6" pad="11"/>
<connect gate="G$1" pin="OUT7" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LDFM50" prefix="U">
<gates>
<gate name="G$1" symbol="VREG"/>
</gates>
<devices>
<device name="" package="DPAK">
<connects>
<connect gate="G$1" pin="GND" pad="TAB"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STD1802T4" prefix="Q">
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="DPAK">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="TAB"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
