<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Displays&lt;/h3&gt;
This library contains LCDs, OLEDs, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LCD-16X2">
<description>&lt;h3&gt;LCD-16x2&lt;/h3&gt;
&lt;p&gt;For Standard hitatchi type LCDs with backlight.  Has 16 pin connection, silk outiline, and mounting holes.&lt;/p&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 16&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area: &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s): 
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/255"&gt;Basic 16x2 LCD&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="LCD-16X2_NOSILK">
<description>&lt;h3&gt;LCD-16x2&lt;/h3&gt;
&lt;p&gt;For Standard hitatchi type LCDs with backlight.  Has 16 pin connection and outline on docu, and mounting holes, but no silkscreen.&lt;/p&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 16&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area: &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s): 
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/255"&gt;Basic 16x2 LCD&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="LCD-16X2_NOHOLESNOSILK">
<description>&lt;h3&gt;LCD-16x2 No silk or mounting holes&lt;/h3&gt;
&lt;p&gt;For Standard hitatchi type LCDs with backlight.  Has 16 pin connection and outline on docu, but no silk or mounting holes.&lt;/p&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 16&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area: &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s): 
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/255"&gt;Basic 16x2 LCD&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="LCD-8X2">
<description>&lt;h3&gt;8x2 Character LCD w/ Backlight&lt;/h3&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 16&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Outer Dimensions: 40.0 x 35.4mm&lt;/li&gt;
&lt;li&gt;Viewing Area: 26.4 x 13.9mm&lt;br&gt;&lt;/li&gt;
&lt;li&gt;Character Size: 2.95 x 4.75mm&lt;br&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s): 
&lt;ul&gt;&lt;li&gt;&lt;a href="http://amotec-display.com/pdf/ADM0802A.pdf"&gt;Amotec Display part ADM0802A PDF&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="LCD-8X2-KIT">
<description>&lt;h3&gt;LCD-8x2 for Kits&lt;/h3&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/ul&gt;&lt;/p&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 16&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Outer Dimensions: 40.0 x 35.4mm&lt;/li&gt;
&lt;li&gt;Viewing Area: 26.4 x 13.9mm&lt;br&gt;&lt;/li&gt;
&lt;li&gt;Character Size: 2.95 x 4.75mm&lt;br&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s): 
&lt;ul&gt;&lt;li&gt;&lt;a href="http://amotec-display.com/pdf/ADM0802A.pdf"&gt;Amotec Display part ADM0802A PDF&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="LCD-G12864">
<description>&lt;h3&gt;G12864&lt;/h3&gt;
&lt;p&gt;For 128x64 LCDs.&lt;/p&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 16&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area: &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s): 
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/255"&gt;Basic 16x2 LCD&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X20">
<description>&lt;h3&gt;0.1" SIL LCD connection&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 20&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1in&lt;/li&gt;
&lt;li&gt;Area: 0.1 x 2.0 in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example Device(s):
&lt;ul&gt;&lt;li&gt;
none
&lt;/p&gt;</description>
</package>
<package name="LCD_BACKLIGHT_PADS">
<description>&lt;h3&gt;Pads for flying backlight leads&lt;/h3&gt;
&lt;p&gt;Generic&lt;/p&gt;</description>
</package>
<package name="NOKIA6100_LCD">
<description>&lt;h3&gt;Nokia 6100 LED Shape and Connector&lt;/h3&gt;
&lt;p&gt;For Nokia-type LCDs.&lt;/p&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 10&lt;/li&gt;
&lt;li&gt;Pin pitch: "&lt;/li&gt;
&lt;li&gt;Area: &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s): 
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/retired/569"&gt;Retired Color LCD&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="OLED-0.66-64X48">
<description>&lt;h3&gt;OLDE display, 0.66 inch&lt;/h3&gt;
&lt;p&gt;For MicroView.&lt;/p&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 28&lt;/li&gt;
&lt;li&gt;Pin pitch: &lt;/li&gt;
&lt;li&gt;Area: &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s): 
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13003"&gt;Microview breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="LCD-16X2_NOSILK-KIT">
<description>&lt;h3&gt;LCD-16x2 for Kits&lt;/h3&gt;
&lt;p&gt;For Standard hitatchi type LCDs with backlight.  Has 16 pin connection and outline on docu, but no silk or mounting holes.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the kit version of the part, so SIL holes are staggered.

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 16&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area: &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s): 
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/255"&gt;Basic 16x2 LCD&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="LCD-16X2_NOSILK-KIT-4BIT">
<description>&lt;h3&gt;LCD-16x2, 4 bit for Kits&lt;/h3&gt;
&lt;p&gt;For Standard hitatchi type LCDs with backlight.  Has a gapped 16-pin connection and outline on docu, but no silk or mounting holes.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the kit version of the part, so SIL holes are staggered.

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 12&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area: &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s): 
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/255"&gt;Basic 16x2 LCD&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="LCD-16X2">
<description>&lt;h3&gt;Standard Character Display Symbol with Standard Backlight&lt;/h3&gt;</description>
<pin name="A" direction="pwr"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="E" direction="in"/>
<pin name="K" direction="pwr"/>
<pin name="R/W" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VO"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="LCD-G12864">
<description>&lt;h3&gt;G12864 Connections&lt;/h3&gt;
&lt;p&gt;This is for the G12864 display.  It is simiar to the standard Hitatchi pinout with additional voltages&lt;/p&gt;</description>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VO"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="CS1" direction="in"/>
<pin name="CS2" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="R/W" direction="in"/>
<pin name="D/I" direction="in"/>
<pin name="E" direction="in"/>
<pin name="VEE"/>
<pin name="A" direction="pwr"/>
<pin name="K" direction="pwr"/>
</symbol>
<symbol name="LCD_BACKLIGHT_PADS">
<description>&lt;h3&gt;General Backlight Connection&lt;/h3&gt;</description>
<pin name="A"/>
<pin name="K"/>
</symbol>
<symbol name="NOKIA6100_LCD">
<description>&lt;h3&gt;Nokia LCD connections&lt;/h3&gt;</description>
<pin name="VDISPLAY"/>
<pin name="VDIGITAL"/>
<pin name="SCK"/>
<pin name="DIO"/>
<pin name="CS"/>
<pin name="GND"/>
<pin name="LEDGND"/>
<pin name="RESET"/>
<pin name="VLED"/>
</symbol>
<symbol name="OLED0.66">
<description>&lt;h3&gt;Micro OLED&lt;/h3&gt;
Monochrome</description>
<pin name="!CS!"/>
<pin name="!RESET!"/>
<pin name="BS1"/>
<pin name="BS2"/>
<pin name="C1N"/>
<pin name="C1P"/>
<pin name="C2N"/>
<pin name="C2P"/>
<pin name="D/!C!"/>
<pin name="D0/SCK"/>
<pin name="D1/MOSI"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="E/!RD!"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="IREF"/>
<pin name="R/!W!"/>
<pin name="VBAT"/>
<pin name="VCC"/>
<pin name="VCOMH"/>
<pin name="VDD"/>
<pin name="VLSS"/>
<pin name="VSS"/>
</symbol>
<symbol name="LCD-16X2-MIN">
<description>&lt;h3&gt;4-bit Character Display Symbol, with RGB backlight&lt;/h3&gt;
&lt;p&gt;This is a somewhat universal part for 16x2 LCDs that have either a white backlight (A/K) or a RGB backlight (RGB+K).&lt;/p&gt;</description>
<pin name="A/K" direction="pwr"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="E" direction="in"/>
<pin name="K/RED" direction="pwr"/>
<pin name="R/W" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VO"/>
<pin name="VSS" direction="pwr"/>
<pin name="GRN" direction="pwr"/>
<pin name="BLU" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LCD-16X2" prefix="LCD">
<description>&lt;h3&gt;Standard text-only 16x2 parallel input LCD&lt;/h3&gt;
&lt;p&gt;Basic 16 character by 2 line display.  Typically utilizes the extremely common HD44780 parallel interface chipset &lt;/p&gt;

&lt;p&gt;SparkFun Products:
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/255"&gt;Basic 16x2 Green&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11122"&gt;Basic 8x2 Green&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LCD-16X2"/>
</gates>
<devices>
<device name="SILK" package="LCD-16X2">
<connects>
<connect gate="G$1" pin="A" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="LCD-00255"/>
</technology>
</technologies>
</device>
<device name="NOSILK" package="LCD-16X2_NOSILK">
<connects>
<connect gate="G$1" pin="A" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="LCD-00255"/>
</technology>
</technologies>
</device>
<device name="NOHOLES" package="LCD-16X2_NOHOLESNOSILK">
<connects>
<connect gate="G$1" pin="A" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="LCD-00255"/>
</technology>
</technologies>
</device>
<device name="8X2" package="LCD-8X2">
<connects>
<connect gate="G$1" pin="A" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="LCD-11122"/>
</technology>
</technologies>
</device>
<device name="8X2-KIT" package="LCD-8X2-KIT">
<connects>
<connect gate="G$1" pin="A" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="R/W" pad="5"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="LCD-11122"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD-G12864" prefix="LCD">
<description>&lt;h3&gt;Graphical LCD 128x64&lt;/h3&gt;
Graphical LCD 644x128 with LED Backlight.
&lt;br&gt;STN Type.
&lt;br&gt; KS0108B parallel interface chipset. 
&lt;br&gt;&lt;a href="https://www.sparkfun.com/datasheets/LCD/GDM12864H.pdf"&gt;Datasheet&lt;/a&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/710"&gt;Graphic LCD 128x64&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LCD-G12864"/>
</gates>
<devices>
<device name="-FULL" package="LCD-G12864">
<connects>
<connect gate="G$1" pin="A" pad="19"/>
<connect gate="G$1" pin="CS1" pad="13"/>
<connect gate="G$1" pin="CS2" pad="12"/>
<connect gate="G$1" pin="D/I" pad="16"/>
<connect gate="G$1" pin="DB0" pad="4"/>
<connect gate="G$1" pin="DB1" pad="5"/>
<connect gate="G$1" pin="DB2" pad="6"/>
<connect gate="G$1" pin="DB3" pad="7"/>
<connect gate="G$1" pin="DB4" pad="8"/>
<connect gate="G$1" pin="DB5" pad="9"/>
<connect gate="G$1" pin="DB6" pad="10"/>
<connect gate="G$1" pin="DB7" pad="11"/>
<connect gate="G$1" pin="E" pad="17"/>
<connect gate="G$1" pin="K" pad="20"/>
<connect gate="G$1" pin="R/W" pad="15"/>
<connect gate="G$1" pin="RST" pad="14"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VEE" pad="18"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="LCD-00710"/>
</technology>
</technologies>
</device>
<device name="-BARE" package="1X20">
<connects>
<connect gate="G$1" pin="A" pad="19"/>
<connect gate="G$1" pin="CS1" pad="13"/>
<connect gate="G$1" pin="CS2" pad="12"/>
<connect gate="G$1" pin="D/I" pad="16"/>
<connect gate="G$1" pin="DB0" pad="4"/>
<connect gate="G$1" pin="DB1" pad="5"/>
<connect gate="G$1" pin="DB2" pad="6"/>
<connect gate="G$1" pin="DB3" pad="7"/>
<connect gate="G$1" pin="DB4" pad="8"/>
<connect gate="G$1" pin="DB5" pad="9"/>
<connect gate="G$1" pin="DB6" pad="10"/>
<connect gate="G$1" pin="DB7" pad="11"/>
<connect gate="G$1" pin="E" pad="17"/>
<connect gate="G$1" pin="K" pad="20"/>
<connect gate="G$1" pin="R/W" pad="15"/>
<connect gate="G$1" pin="RST" pad="14"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VEE" pad="18"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="LCD-00710"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD_BACKLIGHT_PADS">
<description>&lt;h3&gt;Pads for flying backlight leads&lt;/h3&gt;
&lt;p&gt;Use as a place to tack down wires. &lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/"&gt;sparkfun.com&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LCD_BACKLIGHT_PADS"/>
</gates>
<devices>
<device name="" package="LCD_BACKLIGHT_PADS">
<connects>
<connect gate="G$1" pin="A" pad="P$1"/>
<connect gate="G$1" pin="K" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NOKIA6100_LCD" prefix="LCD">
<description>&lt;h3&gt;Nokia 6100 Color LCD&lt;/h3&gt;
&lt;p&gt;

Previously used in production. &lt;/p&gt;

&lt;p&gt;SparkFun Products:
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/retired/569"&gt;128x128 Nokia Knock-Off&lt;/a&gt; (Retired)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/570"&gt;Color LCD SMD connector&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="NOKIA6100_LCD"/>
</gates>
<devices>
<device name="" package="NOKIA6100_LCD">
<connects>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="DIO" pad="3"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="LEDGND" pad="9"/>
<connect gate="G$1" pin="RESET" pad="2"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="VDIGITAL" pad="1"/>
<connect gate="G$1" pin="VDISPLAY" pad="6"/>
<connect gate="G$1" pin="VLED" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="LCD-00570"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OLED0.66" prefix="OLED">
<description>&lt;h3&gt;Micro OLED&lt;/h3&gt;
&lt;p&gt;

&lt;i&gt;TODO: Add description&lt;/i&gt;

&lt;p&gt;SparkFun Products:
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13003"&gt;Micro OLED Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G1" symbol="OLED0.66"/>
</gates>
<devices>
<device name="" package="OLED-0.66-64X48">
<connects>
<connect gate="G1" pin="!CS!" pad="11"/>
<connect gate="G1" pin="!RESET!" pad="12"/>
<connect gate="G1" pin="BS1" pad="9"/>
<connect gate="G1" pin="BS2" pad="10"/>
<connect gate="G1" pin="C1N" pad="5"/>
<connect gate="G1" pin="C1P" pad="4"/>
<connect gate="G1" pin="C2N" pad="3"/>
<connect gate="G1" pin="C2P" pad="2"/>
<connect gate="G1" pin="D/!C!" pad="13"/>
<connect gate="G1" pin="D0/SCK" pad="16"/>
<connect gate="G1" pin="D1/MOSI" pad="17"/>
<connect gate="G1" pin="D2" pad="18"/>
<connect gate="G1" pin="D3" pad="19"/>
<connect gate="G1" pin="D4" pad="20"/>
<connect gate="G1" pin="D5" pad="21"/>
<connect gate="G1" pin="D6" pad="22"/>
<connect gate="G1" pin="D7" pad="23"/>
<connect gate="G1" pin="E/!RD!" pad="15"/>
<connect gate="G1" pin="GND@1" pad="1"/>
<connect gate="G1" pin="GND@2" pad="28"/>
<connect gate="G1" pin="IREF" pad="24"/>
<connect gate="G1" pin="R/!W!" pad="14"/>
<connect gate="G1" pin="VBAT" pad="6"/>
<connect gate="G1" pin="VCC" pad="26"/>
<connect gate="G1" pin="VCOMH" pad="25"/>
<connect gate="G1" pin="VDD" pad="8"/>
<connect gate="G1" pin="VLSS" pad="27"/>
<connect gate="G1" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="LCD-12019"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD-16X2-MIN" prefix="LCD">
<description>&lt;h3&gt;RGB 16x2 parallel input LCD, 4bit only&lt;/h3&gt;
&lt;p&gt;Basic 16 character by 2 line display.  Typically utilizes the extremely common HD44780 parallel interface chipset &lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10862"&gt;Basic 16x2 RGB&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="U1" symbol="LCD-16X2-MIN"/>
</gates>
<devices>
<device name="MIN4-RGB" package="LCD-16X2_NOSILK-KIT-4BIT">
<connects>
<connect gate="U1" pin="A/K" pad="15"/>
<connect gate="U1" pin="BLU" pad="18"/>
<connect gate="U1" pin="DB4" pad="11"/>
<connect gate="U1" pin="DB5" pad="12"/>
<connect gate="U1" pin="DB6" pad="13"/>
<connect gate="U1" pin="DB7" pad="14"/>
<connect gate="U1" pin="E" pad="6"/>
<connect gate="U1" pin="GRN" pad="17"/>
<connect gate="U1" pin="K/RED" pad="16"/>
<connect gate="U1" pin="R/W" pad="5"/>
<connect gate="U1" pin="RS" pad="4"/>
<connect gate="U1" pin="VDD" pad="2"/>
<connect gate="U1" pin="VO" pad="3"/>
<connect gate="U1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="LCD-10862"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
