<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<packages>
<package name="FE1.1S_SSOP-28">
</package>
<package name="USB_TYPE_A_FEMALE_TH">
</package>
</packages>
<symbols>
<symbol name="FE1.1S">
<pin name="VSS"/>
<pin name="VDD5"/>
<pin name="XOUT"/>
<pin name="XIN"/>
<pin name="TESTJ"/>
<pin name="OVCJ"/>
<pin name="PWRJ"/>
<pin name="BUSJ"/>
<pin name="VBUSM"/>
<pin name="XRSTJ"/>
<pin name="DRV"/>
<pin name="LED1"/>
<pin name="LED2"/>
<pin name="VD18_O"/>
<pin name="VD18"/>
<pin name="VD33_O"/>
<pin name="VD33"/>
<pin name="DMU"/>
<pin name="DPU"/>
<pin name="DM4"/>
<pin name="DP4"/>
<pin name="DM3"/>
<pin name="DP3"/>
<pin name="DM2"/>
<pin name="DP2"/>
<pin name="DM1"/>
<pin name="DP1"/>
<pin name="REXT"/>
</symbol>
<symbol name="USB_FEMALE_TYPE_A">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="FE1.1S">
<description>A USB 2.0 hub IC.&lt;br /&gt;&lt;br /&gt;

http://www.jfd-ic.com/Documents/FE1.1s%20Data%20Sheet%20%28Rev.%201.0%29.pdf</description>
<gates>
<gate name="G$1" symbol="FE1.1S"/>
</gates>
<devices>
<device name="" package="FE1.1S_SSOP-28">
<connects>
<connect gate="G$1" pin="BUSJ" pad="19"/>
<connect gate="G$1" pin="DM1" pad="10"/>
<connect gate="G$1" pin="DM2" pad="8"/>
<connect gate="G$1" pin="DM3" pad="6"/>
<connect gate="G$1" pin="DM4" pad="4"/>
<connect gate="G$1" pin="DMU" pad="15"/>
<connect gate="G$1" pin="DP1" pad="11"/>
<connect gate="G$1" pin="DP2" pad="9"/>
<connect gate="G$1" pin="DP3" pad="7"/>
<connect gate="G$1" pin="DP4" pad="5"/>
<connect gate="G$1" pin="DPU" pad="16"/>
<connect gate="G$1" pin="DRV" pad="22"/>
<connect gate="G$1" pin="LED1" pad="23"/>
<connect gate="G$1" pin="LED2" pad="24"/>
<connect gate="G$1" pin="OVCJ" pad="26"/>
<connect gate="G$1" pin="PWRJ" pad="25"/>
<connect gate="G$1" pin="REXT" pad="14"/>
<connect gate="G$1" pin="TESTJ" pad="27"/>
<connect gate="G$1" pin="VBUSM" pad="18"/>
<connect gate="G$1" pin="VD18" pad="28"/>
<connect gate="G$1" pin="VD18_O" pad="12"/>
<connect gate="G$1" pin="VD33" pad="13"/>
<connect gate="G$1" pin="VD33_O" pad="21"/>
<connect gate="G$1" pin="VDD5" pad="20"/>
<connect gate="G$1" pin="VSS" pad="1"/>
<connect gate="G$1" pin="XIN" pad="3"/>
<connect gate="G$1" pin="XOUT" pad="2"/>
<connect gate="G$1" pin="XRSTJ" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_TYPE_A_FEMALE_TH">
<description>USB Type A Female Through Hole.&lt;br /&gt;&lt;br /&gt;

http://datasheet.octopart.com/787616-1-Tyco-Electronics-datasheet-61477.pdf</description>
<gates>
<gate name="G$1" symbol="USB_FEMALE_TYPE_A"/>
</gates>
<devices>
<device name="" package="USB_TYPE_A_FEMALE_TH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
