<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<library>
<packages>
<package name="USB-MICROB">
</package>
<package name="M03X2">
</package>
<package name="M16X1">
</package>
<package name="ETHERNET">
</package>
<package name="FH28-40S-0.5SH(05)">
</package>
<package name="M05X2">
</package>
<package name="M05X2-50MIL_SMD">
</package>
<package name="USB-STACKED">
</package>
<package name="M03X2-50MIL_SMD">
</package>
<package name="M03X2_PADS">
</package>
<package name="3220-10-0300-00">
</package>
<package name="M05X2_SMD">
</package>
<package name="M05X2-100MIL_SHROUD">
</package>
<package name="M07X2-100MIL">
</package>
<package name="M08X2-100MIL_SHROUD">
</package>
<package name="M01X1_100MILX100MIL">
</package>
<package name="M01X1_50MIL">
</package>
<package name="BM10B(0.8)-10DP-0.4V(51)">
</package>
<package name="BM10NB(0.6)-10DS-0.4V(51)">
</package>
<package name="DB9_SMD2">
</package>
<package name="POWERJACK-SMD">
</package>
<package name="USB-A-F-SMD">
</package>
<package name="DOT">
</package>
<package name="M05X2_100MIL-SHROUDED">
</package>
<package name="M10X2-100MIL_SHROUDED">
</package>
<package name="USB-A-MALE-SMT">
</package>
<package name="MFC-OLD">
</package>
<package name="M07X2-100MIL_SHROUD">
</package>
<package name="USB-B-VERTICAL">
</package>
<package name="M04X5">
</package>
<package name="M05X2_50MIL_SHROUDED">
</package>
<package name="35RASMT2BHNTRX">
<description>3.5MM Audio Jack&lt;br&gt;&lt;br&gt;

&lt;a href=http://www.digikey.com/product-detail/en/35RASMT2BHNTRX/SC1489-1-ND/2754494&gt;http://www.digikey.com/product-detail/en/35RASMT2BHNTRX/SC1489-1-ND/2754494&lt;/a&gt;</description>
</package>
<package name="114-00841-68">
<description>&lt;p&gt;Micro SD card slot, Push-In Pull-Out

&lt;p&gt;&lt;a href="http://www.digikey.com/product-detail/en/114-00841-68/114-00841-68-1-ND/2187101"&gt;http://www.digikey.com/product-detail/en/114-00841-68/114-00841-68-1-ND/2187101&lt;/a&gt;</description>
</package>
<package name="M05">
</package>
<package name="DF14A-15P-1.25H(55)">
</package>
<package name="FI-SE20P-HFE">
</package>
<package name="0705530108">
</package>
<package name="TC2030-IDC">
</package>
<package name="TC2030-ICD-NL">
</package>
<package name="1001-011-01101">
</package>
<package name="M18X1">
</package>
<package name="M08X1">
</package>
<package name="0039281083">
</package>
<package name="USB-A-FEMALE">
</package>
<package name="BARREL-POWER_2.1MMX5.5MM">
</package>
<package name="M02-SCREW">
</package>
<package name="M03">
</package>
<package name="RJ11-VERT">
</package>
<package name="BNC-5-1634556-0">
</package>
<package name="9V-NEG">
</package>
<package name="207609-3">
</package>
<package name="M02-POLAR">
</package>
<package name="M03-POLAR">
</package>
<package name="043045-0412">
</package>
<package name="M07X2-100MIL_SHROUD-ALT">
</package>
<package name="0039281043">
</package>
<package name="USB-C-PTH">
</package>
<package name="USB-MICROB2">
</package>
<package name="M05X2-50MIL-SHROUD">
</package>
<package name="10118192-0001LF">
</package>
<package name="M10X1">
</package>
<package name="M10X1-NOSILK">
</package>
<package name="M10X1-SMD">
</package>
<package name="BK-912-G-TR">
</package>
<package name="CWR-170-10-0203">
</package>
<package name="172-E15-113R001">
</package>
<package name="GSB4211311WEU">
</package>
<package name="SMA-PTH">
</package>
<package name="SMA-EDGE">
</package>
<package name="GSB4116341HR">
</package>
<package name="M06X2-PTH-H">
</package>
<package name="BNC-0731000105">
</package>
<package name="M06-PTH-H">
</package>
<package name="0436500212">
</package>
</packages>
<symbols>
<symbol name="POWERJACK">
<pin name="GNDBREAK"/>
<pin name="GND"/>
<pin name="PWR"/>
</symbol>
<symbol name="DOT">
<pin name="P$1"/>
</symbol>
<symbol name="M10X2">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
</symbol>
<symbol name="USB-MICROB">
<pin name="VBUS"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="ID"/>
<pin name="GND"/>
</symbol>
<symbol name="M03X2">
<pin name="1"/>
<pin name="3"/>
<pin name="5"/>
<pin name="6"/>
<pin name="4"/>
<pin name="2"/>
</symbol>
<symbol name="M16X1">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
</symbol>
<symbol name="RB1-125BAG1A">
<pin name="R8"/>
<pin name="R7"/>
<pin name="R2"/>
<pin name="R1"/>
<pin name="R3"/>
<pin name="S$1"/>
<pin name="R6"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="M05X2">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
</symbol>
<symbol name="USB-SHIELD">
<pin name="VBUS"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="GND"/>
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="USB">
<pin name="VBUS"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="GND"/>
</symbol>
<symbol name="M07X2">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
</symbol>
<symbol name="M08X2">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
</symbol>
<symbol name="M01X1">
<pin name="1"/>
</symbol>
<symbol name="SWD">
<pin name="VCC"/>
<pin name="SWDIO"/>
<pin name="SWCLK"/>
<pin name="RESET"/>
<pin name="GND"/>
</symbol>
<symbol name="M09">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
</symbol>
<symbol name="M04X2">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
</symbol>
<symbol name="M04X5-SOLENOID">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
</symbol>
<symbol name="AUDIO">
<pin name="RING"/>
<pin name="L"/>
<pin name="R"/>
</symbol>
<symbol name="MICROSD">
<pin name="CS"/>
<pin name="MOSI"/>
<pin name="GND"/>
<pin name="VDD"/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="CD1"/>
<pin name="CD2"/>
</symbol>
<symbol name="M05">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
</symbol>
<symbol name="M15">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
</symbol>
<symbol name="M20">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
</symbol>
<symbol name="M04">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
</symbol>
<symbol name="M18X1">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
</symbol>
<symbol name="M08">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
</symbol>
<symbol name="M02">
<pin name="1"/>
<pin name="2"/>
</symbol>
<symbol name="M04X2-POWER">
<pin name="5V"/>
<pin name="15V"/>
<pin name="-15V"/>
<pin name="24V"/>
<pin name="AGND"/>
<pin name="PGND"/>
<pin name="GND"/>
</symbol>
<symbol name="M03">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
</symbol>
<symbol name="RJ11-RS232">
<pin name="DTR"/>
<pin name="GND@1"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="GND@2"/>
<pin name="DSR"/>
</symbol>
<symbol name="BNC">
<pin name="GND"/>
<pin name="SIGNAL"/>
</symbol>
<symbol name="BATTERY">
<pin name="P"/>
<pin name="N"/>
</symbol>
<symbol name="M02X2">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
</symbol>
<symbol name="M07X2-INLINE">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
</symbol>
<symbol name="M02X2-POWER">
<pin name="5V"/>
<pin name="24V"/>
<pin name="PGND"/>
<pin name="GND"/>
</symbol>
<symbol name="USB3">
<pin name="SSTX+@1"/>
<pin name="SSTX-@1"/>
<pin name="VBUS@1"/>
<pin name="D+@1"/>
<pin name="D-@1"/>
<pin name="GND@1"/>
<pin name="SSRX-@1"/>
<pin name="SSRX+@1"/>
</symbol>
<symbol name="USBC">
<pin name="SSTX+@1"/>
<pin name="SSTX-@1"/>
<pin name="VBUS@1"/>
<pin name="CC1"/>
<pin name="D+@1"/>
<pin name="D-@1"/>
<pin name="SBU1"/>
<pin name="SBU2"/>
<pin name="CC2"/>
<pin name="SSRX-@2"/>
<pin name="SSRX+@2"/>
<pin name="GND@1"/>
<pin name="VBUS@2"/>
<pin name="GND@2"/>
<pin name="D+@2"/>
<pin name="D-@2"/>
<pin name="VBUS@3"/>
<pin name="VBUS@4"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="SSRX-@1"/>
<pin name="SSRX+@1"/>
<pin name="SSTX-@2"/>
<pin name="SSTX+@2"/>
</symbol>
<symbol name="M10">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
</symbol>
<symbol name="D15">
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
</symbol>
<symbol name="SMA">
<pin name="GND"/>
<pin name="SIGNAL"/>
</symbol>
<symbol name="M06X2">
<pin name="1"/>
<pin name="3"/>
<pin name="5"/>
<pin name="7"/>
<pin name="9"/>
<pin name="11"/>
<pin name="12"/>
<pin name="10"/>
<pin name="8"/>
<pin name="6"/>
<pin name="4"/>
<pin name="2"/>
</symbol>
<symbol name="ARJC02-111008B">
<pin name="P6"/>
<pin name="P4"/>
<pin name="P3"/>
<pin name="P1"/>
<pin name="P2"/>
<pin name="P8"/>
<pin name="P5"/>
</symbol>
<symbol name="ARJC02-111009D">
<pin name="P6"/>
<pin name="P3"/>
<pin name="P2"/>
<pin name="P1"/>
<pin name="P4"/>
<pin name="P8"/>
<pin name="P5"/>
</symbol>
<symbol name="M06">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="POWERJACK" prefix="J">
<gates>
<gate name="G$1" symbol="POWERJACK"/>
</gates>
<devices>
<device name="-SMD1" package="POWERJACK-SMD">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GNDBREAK" pad="2"/>
<connect gate="G$1" pin="PWR" pad="1 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DOT">
<gates>
<gate name="G$1" symbol="DOT"/>
</gates>
<devices>
<device name="" package="DOT">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M10X2" prefix="J">
<gates>
<gate name="G$1" symbol="M10X2"/>
</gates>
<devices>
<device name="-100MIL_SHROUDED" package="M10X2-100MIL_SHROUDED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-MICROB" prefix="J">
<gates>
<gate name="G$1" symbol="USB-MICROB"/>
</gates>
<devices>
<device name="" package="USB-MICROB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND MT1 MT2 P$1 P$2"/>
<connect gate="G$1" pin="ID" pad="ID"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-2" package="USB-MICROB2">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5 P$1 P$2 P$3 P$4"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3" package="10118192-0001LF">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5 P$6 P$7 P$8 P$9 P$10 P$11"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M03X2" prefix="J">
<gates>
<gate name="G$1" symbol="M03X2"/>
</gates>
<devices>
<device name="-PTH" package="M03X2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD" package="M03X2-50MIL_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PADS" package="M03X2_PADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M16X1" prefix="J">
<gates>
<gate name="G$1" symbol="M16X1"/>
</gates>
<devices>
<device name="" package="M16X1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RB1-125BAG1A" prefix="J">
<gates>
<gate name="A" symbol="RB1-125BAG1A"/>
<gate name="GREEN" symbol="LED"/>
<gate name="YELLOW" symbol="LED"/>
</gates>
<devices>
<device name="" package="ETHERNET">
<connects>
<connect gate="A" pin="R1" pad="1"/>
<connect gate="A" pin="R2" pad="2"/>
<connect gate="A" pin="R3" pad="3"/>
<connect gate="A" pin="R6" pad="6"/>
<connect gate="A" pin="R7" pad="7"/>
<connect gate="A" pin="R8" pad="8"/>
<connect gate="A" pin="S$1" pad="P$5 P$6"/>
<connect gate="GREEN" pin="A" pad="10"/>
<connect gate="GREEN" pin="C" pad="9"/>
<connect gate="YELLOW" pin="A" pad="12"/>
<connect gate="YELLOW" pin="C" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M05X2" prefix="J">
<gates>
<gate name="G$1" symbol="M05X2"/>
</gates>
<devices>
<device name="" package="M05X2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-50MIL_SMD-H" package="M05X2-50MIL_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-50MIL_SMD2" package="3220-10-0300-00">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD" package="M05X2_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-100MIL-H" package="M05X2-100MIL_SHROUD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MEZ-H" package="BM10B(0.8)-10DP-0.4V(51)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MEZ-R" package="BM10NB(0.6)-10DS-0.4V(51)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-50MIL_SHROUD" package="M05X2-50MIL-SHROUD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-STACKED" prefix="J">
<gates>
<gate name="A" symbol="USB-SHIELD"/>
<gate name="B" symbol="USB"/>
<gate name="C" symbol="USB"/>
</gates>
<devices>
<device name="" package="USB-STACKED">
<connects>
<connect gate="A" pin="D+" pad="3"/>
<connect gate="A" pin="D-" pad="2"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="P$1" pad="P$1 P$2"/>
<connect gate="A" pin="P$2" pad="P$3 P$4"/>
<connect gate="A" pin="VBUS" pad="1"/>
<connect gate="B" pin="D+" pad="7"/>
<connect gate="B" pin="D-" pad="6"/>
<connect gate="B" pin="GND" pad="8"/>
<connect gate="B" pin="VBUS" pad="5"/>
<connect gate="C" pin="D+" pad="11"/>
<connect gate="C" pin="D-" pad="10"/>
<connect gate="C" pin="GND" pad="12"/>
<connect gate="C" pin="VBUS" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M07X2" prefix="J">
<gates>
<gate name="G$1" symbol="M07X2"/>
</gates>
<devices>
<device name="" package="M07X2-100MIL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-100MIL_SHROUD" package="M07X2-100MIL_SHROUD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M08X2" prefix="J">
<gates>
<gate name="G$1" symbol="M08X2"/>
</gates>
<devices>
<device name="-100MIL_SHROUD" package="M08X2-100MIL_SHROUD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M01X1" prefix="J">
<gates>
<gate name="G$1" symbol="M01X1"/>
</gates>
<devices>
<device name="-100MIL" package="M01X1_100MILX100MIL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-50MIL" package="M01X1_50MIL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWD" prefix="J">
<gates>
<gate name="G$1" symbol="SWD"/>
</gates>
<devices>
<device name="-50MIL" package="3220-10-0300-00">
<connects>
<connect gate="G$1" pin="GND" pad="3 5 9"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="SWCLK" pad="4"/>
<connect gate="G$1" pin="SWDIO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MEZZANINE" package="BM10B(0.8)-10DP-0.4V(51)">
<connects>
<connect gate="G$1" pin="GND" pad="3 5 9"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="SWCLK" pad="4"/>
<connect gate="G$1" pin="SWDIO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-50MIL-SHROUDED" package="M05X2_50MIL_SHROUDED">
<connects>
<connect gate="G$1" pin="GND" pad="3 5 9"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="SWCLK" pad="4"/>
<connect gate="G$1" pin="SWDIO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-50MIL-SHROUDED2" package="M05X2-50MIL-SHROUD">
<connects>
<connect gate="G$1" pin="GND" pad="3 5"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="SWCLK" pad="4"/>
<connect gate="G$1" pin="SWDIO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CARD" package="CWR-170-10-0203">
<connects>
<connect gate="G$1" pin="GND" pad="3 5 9"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="SWCLK" pad="4"/>
<connect gate="G$1" pin="SWDIO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DB9" prefix="J">
<gates>
<gate name="G$1" symbol="M09"/>
</gates>
<devices>
<device name="-SMD2" package="DB9_SMD2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB" prefix="J">
<gates>
<gate name="G$1" symbol="USB-SHIELD"/>
</gates>
<devices>
<device name="-A-MALE-SMT" package="USB-A-MALE-SMT">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$3"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B-VERT" package="USB-B-VERTICAL">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="P$1" pad="P$5 P$7"/>
<connect gate="G$1" pin="P$2" pad="P$6 P$8"/>
<connect gate="G$1" pin="VBUS" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-MALE-SMT2" package="1001-011-01101">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-FEMALE" package="USB-A-FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MFC-OLD" prefix="J">
<gates>
<gate name="G$1" symbol="M04X2"/>
</gates>
<devices>
<device name="" package="MFC-OLD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M04X5" prefix="J">
<gates>
<gate name="G$1" symbol="M04X5-SOLENOID"/>
</gates>
<devices>
<device name="-SOLENOID" package="M04X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO_JACK" prefix="J">
<gates>
<gate name="G$1" symbol="AUDIO"/>
</gates>
<devices>
<device name="" package="35RASMT2BHNTRX">
<connects>
<connect gate="G$1" pin="L" pad="L"/>
<connect gate="G$1" pin="R" pad="R"/>
<connect gate="G$1" pin="RING" pad="RING"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICROSD" prefix="J">
<gates>
<gate name="G$1" symbol="MICROSD"/>
</gates>
<devices>
<device name="-PUSH_PULL" package="114-00841-68">
<connects>
<connect gate="G$1" pin="CD1" pad="CD1"/>
<connect gate="G$1" pin="CD2" pad="CD2"/>
<connect gate="G$1" pin="CS" pad="7"/>
<connect gate="G$1" pin="GND" pad="3 P$1 P$2 P$3 P$4"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MOSI" pad="6"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M05" prefix="J">
<gates>
<gate name="G$1" symbol="M05"/>
</gates>
<devices>
<device name="-PTH" package="M05">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M15" prefix="J">
<gates>
<gate name="G$1" symbol="M15"/>
</gates>
<devices>
<device name="-DF14A-15P-1.25H(55)" package="DF14A-15P-1.25H(55)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M20" prefix="J">
<gates>
<gate name="G$1" symbol="M20"/>
</gates>
<devices>
<device name="-FI-SE20P-HFE" package="FI-SE20P-HFE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M04" prefix="J">
<gates>
<gate name="G$1" symbol="M04"/>
</gates>
<devices>
<device name="-0705530108" package="0705530108">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC2030" prefix="U">
<gates>
<gate name="G$1" symbol="M03X2"/>
</gates>
<devices>
<device name="-IDC" package="TC2030-IDC">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IDC-NL" package="TC2030-ICD-NL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M18X1" prefix="J">
<gates>
<gate name="G$1" symbol="M18X1"/>
</gates>
<devices>
<device name="" package="M18X1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M08X1" prefix="J">
<gates>
<gate name="G$1" symbol="M08"/>
</gates>
<devices>
<device name="" package="M08X1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M04X2" prefix="J">
<gates>
<gate name="G$1" symbol="M04X2"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M04X2-POWER" prefix="J">
<gates>
<gate name="G$1" symbol="M04X2-POWER"/>
</gates>
<devices>
<device name="" package="0039281083">
<connects>
<connect gate="G$1" pin="-15V" pad="2"/>
<connect gate="G$1" pin="15V" pad="1"/>
<connect gate="G$1" pin="24V" pad="7"/>
<connect gate="G$1" pin="5V" pad="6"/>
<connect gate="G$1" pin="AGND" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="PGND" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POWER_JACK" prefix="J">
<gates>
<gate name="G$1" symbol="POWERJACK"/>
</gates>
<devices>
<device name="" package="BARREL-POWER_2.1MMX5.5MM">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GNDBREAK" pad="3"/>
<connect gate="G$1" pin="PWR" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M02" prefix="J">
<gates>
<gate name="G$1" symbol="M02"/>
</gates>
<devices>
<device name="-SCREW" package="M02-SCREW">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-POLAR" package="M02-POLAR">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0436500212" package="0436500212">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ11" prefix="J">
<gates>
<gate name="G$1" symbol="RJ11-RS232"/>
</gates>
<devices>
<device name="-VERT" package="RJ11-VERT">
<connects>
<connect gate="G$1" pin="DSR" pad="6"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="TXD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M03" prefix="J">
<gates>
<gate name="G$1" symbol="M03"/>
</gates>
<devices>
<device name="" package="M03">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LAMP" package="207609-3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-POLAR" package="M03-POLAR">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BNC" prefix="J">
<gates>
<gate name="G$1" symbol="BNC"/>
</gates>
<devices>
<device name="-PTH-H-BULKHEAD" package="BNC-5-1634556-0">
<connects>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4"/>
<connect gate="G$1" pin="SIGNAL" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH-H" package="BNC-0731000105">
<connects>
<connect gate="G$1" pin="GND" pad="P$1 P$2"/>
<connect gate="G$1" pin="SIGNAL" pad="SIGNAL"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATTERY" prefix="B">
<gates>
<gate name="G$1" symbol="BATTERY"/>
</gates>
<devices>
<device name="-9V" package="9V-NEG">
<connects>
<connect gate="G$1" pin="N" pad="N1 N2 N3"/>
<connect gate="G$1" pin="P" pad="P1 P2 P3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="043045-0412" prefix="J">
<gates>
<gate name="G$1" symbol="M02X2"/>
</gates>
<devices>
<device name="" package="043045-0412">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M07X2-ALT" prefix="J">
<gates>
<gate name="G$1" symbol="M07X2-INLINE"/>
</gates>
<devices>
<device name="" package="M07X2-100MIL_SHROUD-ALT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M02X2" prefix="J">
<gates>
<gate name="G$1" symbol="M02X2"/>
</gates>
<devices>
<device name="-I2C" package="043045-0412">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M02X2-POWER" prefix="J">
<gates>
<gate name="G$1" symbol="M02X2-POWER"/>
</gates>
<devices>
<device name="" package="0039281043">
<connects>
<connect gate="G$1" pin="24V" pad="1"/>
<connect gate="G$1" pin="5V" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PGND" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USBC" prefix="J">
<gates>
<gate name="G$1" symbol="USBC"/>
</gates>
<devices>
<device name="-PTH" package="USB-C-PTH">
<connects>
<connect gate="G$1" pin="CC1" pad="A5"/>
<connect gate="G$1" pin="CC2" pad="B5"/>
<connect gate="G$1" pin="D+@1" pad="A6"/>
<connect gate="G$1" pin="D+@2" pad="B6"/>
<connect gate="G$1" pin="D-@1" pad="A7"/>
<connect gate="G$1" pin="D-@2" pad="B7"/>
<connect gate="G$1" pin="GND@1" pad="A1 P$13 P$14 P$15 P$16"/>
<connect gate="G$1" pin="GND@2" pad="A12"/>
<connect gate="G$1" pin="GND@3" pad="B1"/>
<connect gate="G$1" pin="GND@4" pad="B12"/>
<connect gate="G$1" pin="SBU1" pad="A8"/>
<connect gate="G$1" pin="SBU2" pad="B8"/>
<connect gate="G$1" pin="SSRX+@1" pad="B11"/>
<connect gate="G$1" pin="SSRX+@2" pad="A11"/>
<connect gate="G$1" pin="SSRX-@1" pad="B10"/>
<connect gate="G$1" pin="SSRX-@2" pad="A10"/>
<connect gate="G$1" pin="SSTX+@1" pad="A2"/>
<connect gate="G$1" pin="SSTX+@2" pad="B2"/>
<connect gate="G$1" pin="SSTX-@1" pad="A3"/>
<connect gate="G$1" pin="SSTX-@2" pad="B3"/>
<connect gate="G$1" pin="VBUS@1" pad="A4"/>
<connect gate="G$1" pin="VBUS@2" pad="A9"/>
<connect gate="G$1" pin="VBUS@3" pad="B4"/>
<connect gate="G$1" pin="VBUS@4" pad="B9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M10" prefix="J">
<gates>
<gate name="G$1" symbol="M10"/>
</gates>
<devices>
<device name="" package="M10X1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-NOSILK" package="M10X1-NOSILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD" package="M10X1-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT-HLD-001" prefix="B">
<gates>
<gate name="G$1" symbol="BATTERY"/>
</gates>
<devices>
<device name="-NOSILK" package="BK-912-G-TR">
<connects>
<connect gate="G$1" pin="N" pad="-"/>
<connect gate="G$1" pin="P" pad="+1 +2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="D15" prefix="J">
<gates>
<gate name="G$1" symbol="D15"/>
</gates>
<devices>
<device name="-MALE-PTH" package="172-E15-113R001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB3" prefix="J">
<gates>
<gate name="G$1" symbol="USB3"/>
</gates>
<devices>
<device name="-B-PTH" package="GSB4211311WEU">
<connects>
<connect gate="G$1" pin="D+@1" pad="3"/>
<connect gate="G$1" pin="D-@1" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="4 7 P$10 P$11"/>
<connect gate="G$1" pin="SSRX+@1" pad="9"/>
<connect gate="G$1" pin="SSRX-@1" pad="8"/>
<connect gate="G$1" pin="SSTX+@1" pad="6"/>
<connect gate="G$1" pin="SSTX-@1" pad="5"/>
<connect gate="G$1" pin="VBUS@1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-VERT-R" package="GSB4116341HR">
<connects>
<connect gate="G$1" pin="D+@1" pad="3"/>
<connect gate="G$1" pin="D-@1" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="4 7 P$1 P$2 P$3 P$4"/>
<connect gate="G$1" pin="SSRX+@1" pad="6"/>
<connect gate="G$1" pin="SSRX-@1" pad="5"/>
<connect gate="G$1" pin="SSTX+@1" pad="9"/>
<connect gate="G$1" pin="SSTX-@1" pad="8"/>
<connect gate="G$1" pin="VBUS@1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMA" prefix="J" uservalue="yes">
<gates>
<gate name="G$1" symbol="SMA"/>
</gates>
<devices>
<device name="-PTH" package="SMA-PTH">
<connects>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4"/>
<connect gate="G$1" pin="SIGNAL" pad="SIGNAL"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-EDGE" package="SMA-EDGE">
<connects>
<connect gate="G$1" pin="GND" pad="P$1 P$2 P$3 P$4"/>
<connect gate="G$1" pin="SIGNAL" pad="SIGNAL"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M06X2" prefix="J" uservalue="yes">
<gates>
<gate name="G$1" symbol="M06X2"/>
</gates>
<devices>
<device name="-100MIL-H" package="M06X2-PTH-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARJC02-111008B" prefix="J">
<gates>
<gate name="G$1" symbol="ARJC02-111008B"/>
<gate name="YELLOW" symbol="LED"/>
<gate name="GREEN" symbol="LED"/>
</gates>
<devices>
<device name="" package="ETHERNET">
<connects>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P4" pad="4"/>
<connect gate="G$1" pin="P5" pad="5"/>
<connect gate="G$1" pin="P6" pad="6"/>
<connect gate="G$1" pin="P8" pad="8 P$5 P$6"/>
<connect gate="GREEN" pin="A" pad="11"/>
<connect gate="GREEN" pin="C" pad="12"/>
<connect gate="YELLOW" pin="A" pad="9"/>
<connect gate="YELLOW" pin="C" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARJC02-111009D" prefix="J">
<gates>
<gate name="G$1" symbol="ARJC02-111009D"/>
<gate name="_GREEN" symbol="LED"/>
<gate name="_YELLOW" symbol="LED"/>
</gates>
<devices>
<device name="" package="ETHERNET">
<connects>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P4" pad="4"/>
<connect gate="G$1" pin="P5" pad="5"/>
<connect gate="G$1" pin="P6" pad="6"/>
<connect gate="G$1" pin="P8" pad="8 P$5 P$6"/>
<connect gate="_GREEN" pin="A" pad="9"/>
<connect gate="_GREEN" pin="C" pad="10"/>
<connect gate="_YELLOW" pin="A" pad="11"/>
<connect gate="_YELLOW" pin="C" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M06" prefix="J">
<gates>
<gate name="G$1" symbol="M06"/>
</gates>
<devices>
<device name="-PTH-H" package="M06-PTH-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
