<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<library>
<packages>
<package name="SO-8">
</package>
<package name="SOT23-5">
</package>
<package name="SOD123">
</package>
<package name="DPAK">
</package>
<package name="NCP114">
</package>
<package name="SOT23-3">
</package>
<package name="SOD323">
</package>
<package name="SOIC-4">
</package>
</packages>
<symbols>
<symbol name="CAT24M01">
<pin name="VCC"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="GND"/>
<pin name="WP"/>
<pin name="SDA"/>
<pin name="SCL"/>
</symbol>
<symbol name="NCP1400">
<pin name="CE"/>
<pin name="OUT"/>
<pin name="GND"/>
<pin name="LX"/>
</symbol>
<symbol name="SCHOTTKY">
<pin name="A"/>
<pin name="C"/>
</symbol>
<symbol name="MOSFET-N">
<pin name="GATE"/>
<pin name="SOURCE"/>
<pin name="DRAIN"/>
</symbol>
<symbol name="VREG">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="BRIDGE-RECTIFIER">
<pin name="+"/>
<pin name="-"/>
<pin name="AC@1"/>
<pin name="AC@2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CAT24M01" prefix="U">
<description>&lt;b&gt; 1Mb  I2C CMOS EEPROM &lt;b&gt;</description>
<gates>
<gate name="G$1" symbol="CAT24M01"/>
</gates>
<devices>
<device name="" package="SO-8">
<connects>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1400" prefix="U">
<gates>
<gate name="G$1" symbol="NCP1400"/>
</gates>
<devices>
<device name="ASN50T1G" package="SOT23-5">
<connects>
<connect gate="G$1" pin="CE" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LX" pad="5"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MBR0520" prefix="D">
<gates>
<gate name="G$1" symbol="SCHOTTKY"/>
</gates>
<devices>
<device name="LT1G" package="SOD123">
<connects>
<connect gate="G$1" pin="A" pad="ANODE"/>
<connect gate="G$1" pin="C" pad="CATHODE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NTD5806" prefix="U">
<description>40V N-Channel Mosfet 33A continuous current, Vgs 2.5V @ 250uA</description>
<gates>
<gate name="G$1" symbol="MOSFET-N"/>
</gates>
<devices>
<device name="NT4G" package="DPAK">
<connects>
<connect gate="G$1" pin="DRAIN" pad="TAB"/>
<connect gate="G$1" pin="GATE" pad="1"/>
<connect gate="G$1" pin="SOURCE" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NTD5867" prefix="Q">
<gates>
<gate name="G$1" symbol="MOSFET-N"/>
</gates>
<devices>
<device name="NLT4G" package="DPAK">
<connects>
<connect gate="G$1" pin="DRAIN" pad="TAB"/>
<connect gate="G$1" pin="GATE" pad="1"/>
<connect gate="G$1" pin="SOURCE" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1117" prefix="U">
<gates>
<gate name="G$1" symbol="VREG"/>
</gates>
<devices>
<device name="DT12G" package="DPAK">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="TAB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2N7002" prefix="Q">
<gates>
<gate name="G$1" symbol="MOSFET-N"/>
</gates>
<devices>
<device name="LT1G" package="SOT23-3">
<connects>
<connect gate="G$1" pin="DRAIN" pad="3"/>
<connect gate="G$1" pin="GATE" pad="1"/>
<connect gate="G$1" pin="SOURCE" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NSR0530" prefix="D">
<gates>
<gate name="G$1" symbol="SCHOTTKY"/>
</gates>
<devices>
<device name="HT1G" package="SOD323">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MB6S" prefix="D">
<gates>
<gate name="G$1" symbol="BRIDGE-RECTIFIER"/>
</gates>
<devices>
<device name="" package="SOIC-4">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
<connect gate="G$1" pin="AC@1" pad="3"/>
<connect gate="G$1" pin="AC@2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
