<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle>
    <drawing>
        <library name="Upverter Library">
            <description>Upverter Parts Library

Created by Upverter.com</description>
            <packages>
                <package name="TEXAS_INSTRUMENTS_PGA4311U_0">
                    <description>Audio Volume Control 4 Channel 28-SOIC</description>
                </package>
            </packages>
            <symbols>
                <symbol name="TEXAS_INSTRUMENTS_PGA4311U_0_0">
                    <description>Audio Volume Control 4 Channel 28-SOIC</description>
                    <pin name="AIN_1"/>
                    <pin name="AIN_2"/>
                    <pin name="AIN_3"/>
                    <pin name="AIN_4"/>
                    <pin name="AOUT_1"/>
                    <pin name="AOUT_2"/>
                    <pin name="AOUT_3"/>
                    <pin name="AOUT_4"/>
                    <pin name="1_VA+"/>
                    <pin name="2_VA+"/>
                    <pin name="1_VA−"/>
                    <pin name="2_VA−"/>
                    <pin name="!CS!"/>
                    <pin name="!MUTE!"/>
                    <pin name="SCLK"/>
                    <pin name="SDI"/>
                    <pin name="SDO"/>
                    <pin name="VD+"/>
                    <pin name="ZCEN"/>
                    <pin name="1_AGND_1"/>
                    <pin name="2_AGND_1"/>
                    <pin name="1_AGND_2"/>
                    <pin name="2_AGND_2"/>
                    <pin name="1_AGND_3"/>
                    <pin name="2_AGND_3"/>
                    <pin name="1_AGND_4"/>
                    <pin name="2_AGND_4"/>
                    <pin name="DGND"/>
                </symbol>
            </symbols>
            <devicesets>
                <deviceset prefix="U" name="TEXAS_INSTRUMENTS_PGA4311U">
                    <description>Audio Volume Control 4 Channel 28-SOIC</description>
                    <gates>
                        <gate name="G$0" symbol="TEXAS_INSTRUMENTS_PGA4311U_0_0"/>
                    </gates>
                    <devices>
                        <device name="TEXAS_INSTRUMENTS_PGA4311U_0_0" package="TEXAS_INSTRUMENTS_PGA4311U_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="!MUTE!"/>
                                <connect gate="G$0" pad="2" pin="1_AGND_1"/>
                                <connect gate="G$0" pad="3" pin="AIN_1"/>
                                <connect gate="G$0" pad="4" pin="2_AGND_1"/>
                                <connect gate="G$0" pad="5" pin="AOUT_1"/>
                                <connect gate="G$0" pad="6" pin="1_VA−"/>
                                <connect gate="G$0" pad="7" pin="1_VA+"/>
                                <connect gate="G$0" pad="8" pin="AOUT_3"/>
                                <connect gate="G$0" pad="9" pin="1_AGND_3"/>
                                <connect gate="G$0" pad="10" pin="AIN_3"/>
                                <connect gate="G$0" pad="11" pin="2_AGND_3"/>
                                <connect gate="G$0" pad="12" pin="VD+"/>
                                <connect gate="G$0" pad="13" pin="SDI"/>
                                <connect gate="G$0" pad="14" pin="!CS!"/>
                                <connect gate="G$0" pad="15" pin="SCLK"/>
                                <connect gate="G$0" pad="16" pin="SDO"/>
                                <connect gate="G$0" pad="17" pin="DGND"/>
                                <connect gate="G$0" pad="18" pin="1_AGND_4"/>
                                <connect gate="G$0" pad="19" pin="AIN_4"/>
                                <connect gate="G$0" pad="20" pin="2_AGND_4"/>
                                <connect gate="G$0" pad="21" pin="AOUT_4"/>
                                <connect gate="G$0" pad="22" pin="2_VA+"/>
                                <connect gate="G$0" pad="23" pin="2_VA−"/>
                                <connect gate="G$0" pad="24" pin="AOUT_2"/>
                                <connect gate="G$0" pad="25" pin="1_AGND_2"/>
                                <connect gate="G$0" pad="26" pin="AIN_2"/>
                                <connect gate="G$0" pad="27" pin="2_AGND_2"/>
                                <connect gate="G$0" pad="28" pin="ZCEN"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="595-PGA4311U"/>
                                    <attribute name="description" value="Audio Volume Control 4 Channel 28-SOIC"/>
                                    <attribute name="temperature_range_high" value="+85°C"/>
                                    <attribute name="MPN" value="PGA4311U"/>
                                    <attribute name="digikey_description" value="IC VOLUME CTRL AUD 4-CH 28-SOIC"/>
                                    <attribute name="digikey_part_number" value="PGA4311U-ND"/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="datasheet" value="http://www.ti.com/lit/ds/symlink/pga4311.pdf"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="mfg_package_ident" value="DW (R-PDSO-G28)"/>
                                    <attribute name="voltage" value=""/>
                                    <attribute name="temperature_range_low" value="-40°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="MF" value="Texas Instruments"/>
                                    <attribute name="package" value="SOP28"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
            </devicesets>
        </library>
    </drawing>
</eagle>
